# `colorsys` — Conversions between color systems

소스 코드: Lib/colorsys.py

The `colorsys` module defines bidirectional conversions of color values between colors expressed in the RGB (Red Green Blue) color space used in computer monitors and three other coordinate systems: YIQ, HLS (Hue Lightness Saturation) and HSV (Hue Saturation Value). Coordinates in all of these color spaces are floating point values. In the YIQ space, the Y coordinate is between 0 and 1, but the I and Q coordinates can be positive or negative. In all other spaces, the coordinates are all between 0 and 1.

더 보기

색 공간에 대한 자세한 내용은 https://poynton.ca/ColorFAQ.html 와 https://www.cambridgeincolour.com/tutorials/color-spaces.htm 에서 확인할 수 있습니다.

`colorsys` 모듈은 다음 함수를 정의합니다:

colorsys.rgb_to_yiq(r, g, b)

  RGB 좌표에서 YIQ 좌표로 색을 변환합니다.

colorsys.yiq_to_rgb(y, i, q)

  YIQ 좌표에서 RGB 좌표로 색을 변환합니다.

colorsys.rgb_to_hls(r, g, b)

  RGB 좌표에서 HLS 좌표로 색을 변환합니다.

colorsys.hls_to_rgb(h, l, s)

  HLS 좌표에서 RGB 좌표로 색을 변환합니다.

colorsys.rgb_to_hsv(r, g, b)

  RGB 좌표에서 HSV 좌표로 색을 변환합니다.

colorsys.hsv_to_rgb(h, s, v)

  HSV 좌표에서 RGB 좌표로 색을 변환합니다.

예:

    >>> import colorsys
    >>> colorsys.rgb_to_hsv(0.2, 0.4, 0.4)
    (0.5, 0.5, 0.4)
    >>> colorsys.hsv_to_rgb(0.5, 0.5, 0.4)
    (0.2, 0.4, 0.4)